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	Re   Region: Asia Pacific-Hong Kong


Project: 2008 Olympic Horse Competition Lagoon, HK Jockey Club
Product: Bentofix
Client: HK Jockey Club

Main Contractors: Uni-Bright Engineering Ltd
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The high quality Bentofix Lake Liner is a Germany made shear strength transmitting GCL, consists of a continuous layer of natural sodium bentonite, sandwiched between a needle-punched nonwoven polypropylene (PP) geotextile (cover layer) and a slit film woven (PP) geotextile (carrier layer). The components are needle-punched uniformly together across the entire membrane. A second layer of bentonite with the same quality as the central bentonite layer is impregnated into the nonwoven component to facilitate impermeable overlap joints. These sophisticated processes make Bentofix into a 4-in-1 layered GCL.

Bentofix uses powdered natural sodium bentonite which enables a homogeneous coverage of the lake. The small particle size of the powdered bentonite reacts immediately to the presence of water, drastically reducing the activation time of the bentonite. On site this means an immediate waterproofing ability.
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